(footprint "Diode_Bridge_Round_D8.9mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "4-lead round diode bridge package, diameter 8.9mm, pin pitch 5.08mm, see http://cdn-reichelt.de/documents/datenblatt/A400/W005M-W10M_SEP.PDF")
	(tags "diode bridge 8.9mm 8.85mm WOB pitch 5.08mm")
	(property "Reference" "REF**"
		(at 2.54 -2.794 0)
		(layer "F.SilkS")
	)
	(property "Value" "Diode_Bridge_Round_D8.9mm"
		(at 2.794 8.128 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 3.81 2.54 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 0 5.08)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 5.08 5.08)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 5.08 0)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/Diode_Bridge_Round_D8.9mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
