(footprint "AG12864E"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "STN/FSTN LCD 128x64 dot https://www.digchip.com/datasheets/parts/datasheet/1121/AG-12864E-pdf.php")
	(tags "AG12864E Graphics Display 128x64 Ampire")
	(property "Reference" "REF**"
		(at -0.4 -14.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "AG12864E"
		(at 46 -14.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 24.6 23.4 0)
		(layer "F.Fab")
	)
	(pad "" thru_hole circle
		(at 0 -10.87 270)
		(size 3.2 3.2)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at 0 59.13 270)
		(size 3.2 3.2)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at 49.7 -10.87 270)
		(size 3.2 3.2)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at 49.7 59.13 270)
		(size 3.2 3.2)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at 0 0 270)
		(size 1.8 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 0 2.54 270)
		(size 1.8 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 0 5.08 270)
		(size 1.8 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 0 7.62 270)
		(size 1.8 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 0 10.16 270)
		(size 1.8 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 0 12.7 270)
		(size 1.8 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole oval
		(at 0 15.24 270)
		(size 1.8 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole oval
		(at 0 17.78 270)
		(size 1.8 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole oval
		(at 0 20.32 270)
		(size 1.8 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole oval
		(at 0 22.86 270)
		(size 1.8 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole oval
		(at 0 25.4 270)
		(size 1.8 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole oval
		(at 0 27.94 270)
		(size 1.8 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole oval
		(at 0 30.48 270)
		(size 1.8 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole oval
		(at 0 33.02 270)
		(size 1.8 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole oval
		(at 0 35.56 270)
		(size 1.8 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole oval
		(at 0 38.1 270)
		(size 1.8 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole oval
		(at 0 40.64 270)
		(size 1.8 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" thru_hole oval
		(at 0 43.18 270)
		(size 1.8 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "19" thru_hole oval
		(at 0 45.72 270)
		(size 1.8 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "20" thru_hole oval
		(at 0 48.26 270)
		(size 1.8 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Display.3dshapes/AG12864E.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
