(footprint "ER-OLED0.42-1W_Folded"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "72x40 white graphic OLED display 0.42 inch, SSD1306B controller, I2C and SPI, folded back https://www.buydisplay.com/download/manual/ER-OLED0.42-1_Datasheet.pdf")
	(tags "SSD1306 OLED display 0.42 inch")
	(property "Reference" "REF**"
		(at 0 9.45 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "ER-OLED0.42-1W_Folded"
		(at 0 12 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 -0.25 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 -0.25 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 9.45 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -4.875 0 90)
		(size 2.5 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -4.225 0 90)
		(size 2.5 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -3.575 0 90)
		(size 2.5 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -2.925 0 90)
		(size 2.5 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -2.275 0 90)
		(size 2.5 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -1.625 0 90)
		(size 2.5 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -0.975 0 90)
		(size 2.5 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -0.325 0 90)
		(size 2.5 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 0.325 0 90)
		(size 2.5 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 0.975 0 90)
		(size 2.5 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 1.625 0 90)
		(size 2.5 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 2.275 0 90)
		(size 2.5 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 2.925 0 90)
		(size 2.5 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 3.575 0 90)
		(size 2.5 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at 4.225 0 90)
		(size 2.5 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at 4.875 0 90)
		(size 2.5 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Display.3dshapes/ER-OLED0.42-1W_Folded.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
