(footprint "HDSM-441B_HDSM-443B"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "2 Digit 7 segemnt blue LED, right hand decimal, https://docs.broadcom.com/docs/AV02-1589EN")
	(tags "2 Digit 7 segment blue LED")
	(property "Reference" "REF**"
		(at -7.21 -10.77 0)
		(layer "F.SilkS")
	)
	(property "Value" "HDSM-441B_HDSM-443B"
		(at 0.18 11.02 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.61 -0.03 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -7.5 -5.08 270)
		(size 2 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -7.5 -2.54 270)
		(size 2 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -7.5 0 270)
		(size 2 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -7.5 2.54 270)
		(size 2 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -7.5 5.08 270)
		(size 2 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 7.5 5.08 270)
		(size 2 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 7.5 2.54 270)
		(size 2 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 7.5 0 270)
		(size 2 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 7.5 -2.54 270)
		(size 2 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 7.5 -5.08 270)
		(size 2 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Display.3dshapes/HDSM-441B_HDSM-443B.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
