(footprint "HDSP-4836"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "10-Element Red Yellow Green Bar Graph Array https://docs.broadcom.com/docs/AV02-1798EN")
	(tags "10-Element Red Yellow Green Bar Graph Array")
	(property "Reference" "REF**"
		(at 0.45 -2.42 0)
		(layer "F.SilkS")
	)
	(property "Value" "HDSP-4836"
		(at 2.86 25.2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 4 12 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 2.54 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 5.08 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0 7.62 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 0 10.16 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 0 12.7 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 0 15.24 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 0 17.78 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 0 20.32 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 0 22.86 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 7.62 22.86 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 7.62 20.32 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 7.62 17.78 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 7.62 15.24 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at 7.62 12.7 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole circle
		(at 7.62 10.16 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 7.62 7.62 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" thru_hole circle
		(at 7.62 5.08 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "19" thru_hole circle
		(at 7.62 2.54 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "20" thru_hole circle
		(at 7.62 0 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Display.3dshapes/HDSP-4836.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
