(footprint "LM16255"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "LCD LM16255 16x2 character http://www.datasheetlib.com/datasheet/259542/lm16255_sharp-electronics.html")
	(tags "LCD 12x2")
	(property "Reference" "REF**"
		(at -38.83 -3.91 0)
		(layer "F.SilkS")
	)
	(property "Value" "LM16255"
		(at -37.82 42.57 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0.23 21.15 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -38.28 37.46 180)
		(size 2.5 2.5)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -36.78 1.46 180)
		(size 2.5 2.5)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 39.22 1.46 180)
		(size 2.5 2.5)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 40.72 37.46 180)
		(size 2.5 2.5)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0 180)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 2.54 0 180)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 5.08 0 180)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 7.62 0 180)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 10.16 0 180)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 12.7 0 180)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 15.24 0 180)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 17.78 0 180)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 20.32 0 180)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 22.86 0 180)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 25.4 0 180)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 27.94 0 180)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 30.48 0 180)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 33.02 0 180)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Display.3dshapes/LM16255.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
