(footprint "AD-121F2"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Single Digit 7-segment RGB LED Display, 1-inch digit height, common anode, http://usasyck.com/products/AD-121F2_cat_e.pdf")
	(tags "RGB LED digit")
	(property "Reference" "REF**"
		(at 15 -4.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "AD-121F2"
		(at 15 22 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 15 8.75 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -2.25 -2.75)
		(size 1.45 1.45)
		(drill 1.45)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 32.25 20.25)
		(size 1.45 1.45)
		(drill 1.45)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.7 1.7)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 2.5)
		(size 1.7 1.7)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 5)
		(size 1.7 1.7)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0 7.5)
		(size 1.7 1.7)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 0 10)
		(size 1.7 1.7)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 0 12.5)
		(size 1.7 1.7)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 2.5 0)
		(size 1.7 1.7)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 2.5 2.5)
		(size 1.7 1.7)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 2.5 12.5)
		(size 1.7 1.7)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 27.5 0)
		(size 1.7 1.7)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 27.5 2.5)
		(size 1.7 1.7)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at 27.5 5)
		(size 1.7 1.7)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole circle
		(at 27.5 15)
		(size 1.7 1.7)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 27.5 17.5)
		(size 1.7 1.7)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" thru_hole circle
		(at 30 0)
		(size 1.7 1.7)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "19" thru_hole circle
		(at 30 2.5)
		(size 1.7 1.7)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "20" thru_hole circle
		(at 30 5)
		(size 1.7 1.7)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 30 7.5)
		(size 1.7 1.7)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" thru_hole circle
		(at 30 10)
		(size 1.7 1.7)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "23" thru_hole circle
		(at 30 12.5)
		(size 1.7 1.7)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "24" thru_hole circle
		(at 30 15)
		(size 1.7 1.7)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at 30 17.5)
		(size 1.7 1.7)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Display_7Segment.3dshapes/AD-121F2.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
