(footprint "AFF_2x7SEG-DIGIT_10mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Afficheur 7 segments 10mm DIGIT")
	(tags "AFFICHEUR")
	(property "Reference" "REF**"
		(at 7.5 -3.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "AFF_2x7SEG-DIGIT_10mm"
		(at 4.5 9.25 270)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 7.25 8.25 270)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 2.54 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 5.08 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0 7.62 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 0 10.16 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 0 12.7 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 0 15.24 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 0 17.78 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 15.24 17.78 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 15.24 15.24 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 15.24 12.7 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 15.24 10.16 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 15.24 7.62 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 15.24 5.08 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at 15.24 2.54 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole circle
		(at 15.24 0 270)
		(size 2.032 2.032)
		(drill 0.9144)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
)
