(footprint "LairdTech_28C0236-0JW-10"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Ferrite, vertical, LairdTech 28C0236-0JW-10, https://assets.lairdtech.com/home/brandworld/files/28C0236-0JW-10.pdf, JW Miller core https://www.bourns.com/products/magnetic-products/j.w.-miller-through-hole-ferrite-beads-emi-filters")
	(tags "Ferrite vertical LairdTech 28C0236-0JW-10")
	(property "Reference" "REF**"
		(at 2.54 -4.064 0)
		(layer "F.SilkS")
	)
	(property "Value" "LairdTech_28C0236-0JW-10"
		(at 2.54 4.953 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.54 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2 2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 5.08 0)
		(size 2 2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Ferrite_THT.3dshapes/LairdTech_28C0236-0JW-10.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
