(footprint "Fiducial_1mm_Mask3mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Circular Fiducial, 1mm bare copper, 3mm soldermask opening (recommended)")
	(tags "fiducial")
	(property "Reference" "REF**"
		(at 0 -2.54 0)
		(layer "F.SilkS")
	)
	(property "Value" "Fiducial_1mm_Mask3mm"
		(at 0 2.286 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd circle
		(at 0 0)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 1)
		(clearance 1)
	)
	(embedded_fonts no)
)
