(footprint "Filter_1109-5_1.1x0.9mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "5-pin SAW filter package - 1.1x0.9 mm Body; (see https://www.murata.com/~/media/webrenewal/support/library/catalog/products/filter/rf/p73e.ashx?la=en-gb)")
	(tags "Filter 5")
	(property "Reference" "REF**"
		(at 0 1.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "Filter_1109-5_1.1x0.9mm"
		(at 0 -1.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -2.7 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -0.385 0 90)
		(size 0.25 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0 0.25 90)
		(size 0.25 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0.385 0.25 90)
		(size 0.25 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 0.385 -0.25 90)
		(size 0.25 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 0 -0.25 90)
		(size 0.25 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Filter.3dshapes/Filter_1109-5_1.1x0.9mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
