(footprint "Filter_Mini-Circuits_FV1206-6"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Mini-Circuits Filter SMD 1206 https://ww2.minicircuits.com/case_style/FV1206-6.pdf")
	(tags "Mini-Circuits Filter SMD 1206")
	(property "Reference" "REF**"
		(at 0 -2.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "Filter_Mini-Circuits_FV1206-6"
		(at 0 2.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -1.715 0)
		(size 0.99 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -0.99 1.06625)
		(size 0.65 1.2125)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" thru_hole circle
		(at -0.99 1.51)
		(size 0.65 0.65)
		(drill 0.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" smd roundrect
		(at 0 1.06625)
		(size 0.65 1.2125)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" thru_hole circle
		(at 0 1.51)
		(size 0.65 0.65)
		(drill 0.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" smd roundrect
		(at 0.99 1.06625)
		(size 0.65 1.2125)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" thru_hole circle
		(at 0.99 1.51)
		(size 0.65 0.65)
		(drill 0.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" smd roundrect
		(at 1.715 0)
		(size 0.99 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" thru_hole circle
		(at 0.99 -1.51)
		(size 0.65 0.65)
		(drill 0.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" smd roundrect
		(at 0.99 -1.06625)
		(size 0.65 1.2125)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" thru_hole circle
		(at 0 -1.51)
		(size 0.65 0.65)
		(drill 0.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" smd roundrect
		(at 0 -1.06625)
		(size 0.65 1.2125)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" thru_hole circle
		(at -0.99 -1.51)
		(size 0.65 0.65)
		(drill 0.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" smd roundrect
		(at -0.99 -1.06625)
		(size 0.65 1.2125)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Filter.3dshapes/Filter_Mini-Circuits_FV1206-6.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
