(footprint "Filter_Murata_BNX025_ThermalVias"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://www.murata.com/en-us/products/productdata/8796778004510/QNFH9101.pdf?1496719830000")
	(tags "EMI Filter")
	(property "Reference" "REF**"
		(at -4.4 -5.65 180)
		(layer "F.SilkS")
	)
	(property "Value" "Filter_Murata_BNX025_ThermalVias"
		(at 0 11.2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.75 -0.05 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -6.85 -2.15)
		(size 3.8 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 6.85 -2.15)
		(size 3.8 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 0.5)
	)
	(pad "3" smd rect
		(at -6.85 2.15)
		(size 3.8 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" thru_hole circle
		(at -1.25 -9.65)
		(size 1.524 1.524)
		(drill 0.8)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at -1.25 -5.15)
		(size 1.524 1.524)
		(drill 0.8)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at -1.25 0)
		(size 1.524 1.524)
		(drill 0.8)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at -1.25 5.05)
		(size 1.524 1.524)
		(drill 0.8)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at -1.25 9.55)
		(size 1.524 1.524)
		(drill 0.8)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" smd rect
		(at 0.35 -5.3)
		(size 8.2 10.6)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "4" smd rect
		(at 1 5.05)
		(size 7.9 2.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at 3 -9.65)
		(size 1.524 1.524)
		(drill 0.8)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at 3.25 -5.15)
		(size 1.524 1.524)
		(drill 0.8)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" smd rect
		(at 3.25 -5.15)
		(size 3.4 2.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at 3.25 0)
		(size 1.524 1.524)
		(drill 0.8)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at 3.25 5.05)
		(size 1.524 1.524)
		(drill 0.8)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" smd rect
		(at 3.25 5.25)
		(size 14 10.5)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at 3.25 9.55)
		(size 1.524 1.524)
		(drill 0.8)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" smd rect
		(at 6.85 2.15)
		(size 3.8 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at 7.75 5.05)
		(size 1.524 1.524)
		(drill 0.8)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Filter.3dshapes/Filter_Murata_BNX025.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
