(footprint "Filter_Murata_SFECF-6"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SMD Type 10.7MHz Ceramic Filter https://www.murata.com/en-us/products/filter/cerafil/sfecf")
	(tags "10.7MHz smd ceramic")
	(property "Reference" "REF**"
		(at 0 -2.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Filter_Murata_SFECF-6"
		(at 0 2.48 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -1.225 -1.4)
		(size 1.05 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.0625)
	)
	(pad "2" smd roundrect
		(at -1.225 0)
		(size 1.05 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.0625)
	)
	(pad "3" smd roundrect
		(at -1.225 1.4)
		(size 1.05 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.0625)
	)
	(pad "4" smd roundrect
		(at 1.225 1.4)
		(size 1.05 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.0625)
	)
	(pad "5" smd roundrect
		(at 1.225 0)
		(size 1.05 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.0625)
	)
	(pad "6" smd roundrect
		(at 1.225 -1.4)
		(size 1.05 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.0625)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Filter.3dshapes/Filter_Murata_SFECF-6.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
