(footprint "Filter_SAW-6_3.8x3.8mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "6-pin 3.8 x 3.8mm SAW filter package, https://www.golledge.com/media/3785/mp08167.pdf")
	(tags "SAW filter 6-pin")
	(property "Reference" "REF**"
		(at 0.01 3.22 0)
		(layer "F.SilkS")
	)
	(property "Value" "Filter_SAW-6_3.8x3.8mm"
		(at 0.01 -3.09 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at -0.02 0.01 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -0.9 -1.27)
		(size 2.2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.4 0)
		(size 1.2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.4 1.27)
		(size 1.2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 1.4 1.27)
		(size 1.2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.4 0)
		(size 1.2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.4 -1.27)
		(size 1.2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Filter.3dshapes/Filter_SAW-6_3.8x3.8mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
