(footprint "Fuse_Bourns_TBU-CA"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Bourns TBU-CA Fuse, 2 Pin (https://www.bourns.com/data/global/pdfs/TBU-CA.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "Bourns Fuse NoLead")
	(property "Reference" "REF**"
		(at 0 -2.95 0)
		(layer "F.SilkS")
	)
	(property "Value" "Fuse_Bourns_TBU-CA"
		(at 0 2.95 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -2.025 0)
		(size 2 3.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "2" smd rect
		(at 0 0)
		(size 0.8 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd roundrect
		(at 2.025 0)
		(size 2 3.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Fuse.3dshapes/Fuse_Bourns_TBU-CA.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
