(footprint "Fuseholder_Blade_ATO_Littelfuse_Pudenz_2_Pin"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Fuseholder ATO Blade littelfuse Pudenz 2 Pin")
	(tags "Fuseholder ATO Blade littelfuse Pudenz 2 Pin")
	(property "Reference" "REF**"
		(at 4.57 -2.78 0)
		(layer "F.SilkS")
	)
	(property "Value" "Fuseholder_Blade_ATO_Littelfuse_Pudenz_2_Pin"
		(at 5.07 5.22 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 4.5 3.5 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 4.6 1.2)
		(size 2.4 2.4)
		(drill 2.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 3.5 3.5)
		(drill 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 9.2 0)
		(size 3.5 3.5)
		(drill 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Fuse.3dshapes/Fuseholder_Blade_ATO_Littelfuse_Pudenz_2_Pin.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
