(footprint "Fuseholder_Clip-5x20mm_Littelfuse_520_Inline_P20.50x5.80mm_D1.30mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Fuseholder Clips, 5x20mm Cylinder Fuse, Pins Inline, Horizontal, Littelfuse 520, https://m.littelfuse.com/~/media/electronics/datasheets/fuse_clips/littelfuse_fuse_clip_100_445_030_520_datasheet.pdf.pdf")
	(tags "fuse clip open")
	(property "Reference" "REF**"
		(at 10.25 -4 0)
		(layer "F.SilkS")
	)
	(property "Value" "Fuseholder_Clip-5x20mm_Littelfuse_520_Inline_P20.50x5.80mm_D1.30mm_Horizontal"
		(at 10.25 4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 10.25 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "1" thru_hole roundrect
		(at 5.8 0)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "2" thru_hole circle
		(at 14.7 0)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 20.5 0)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Fuse.3dshapes/Fuseholder_Clip-5x20mm_Littelfuse_520_Inline_P20.50x5.80mm_D1.30mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
