(footprint "Fuseholder_Clip-6.3x32mm_Littelfuse_102_Inline_P34.21x7.62mm_D2.54mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Fuseholder Clips, 6.3x32mm Cylinder Fuse, Pins Inline, Horizontal, Littelfuse 102 Bowed Leads, https://www.littelfuse.com/~/media/electronics/datasheets/fuse_clips/littelfuse_fuse_clip_102_122_datasheet.pdf.pdf")
	(tags "fuse clip open")
	(property "Reference" "REF**"
		(at 17.1 -5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Fuseholder_Clip-6.3x32mm_Littelfuse_102_Inline_P34.21x7.62mm_D2.54mm_Horizontal"
		(at 17.1 5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 17.1 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 3.5 3.5)
		(drill 2.54)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "1" thru_hole roundrect
		(at 7.62 0)
		(size 3.5 3.5)
		(drill 2.54)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "2" thru_hole circle
		(at 26.59 0)
		(size 3.5 3.5)
		(drill 2.54)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 34.21 0)
		(size 3.5 3.5)
		(drill 2.54)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Fuse.3dshapes/Fuseholder_Clip-6.3x32mm_Littelfuse_102_Inline_P34.21x7.62mm_D2.54mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
