(footprint "Fuseholder_Cylinder-5x20mm_Bulgin_FX0456_Vertical_Closed"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Fuseholder, 5x20, closed, vertical, Bulgin, FX0456, https://www.bulgin.com/products/pub/media/bulgin/data/Fuseholders.pdf")
	(tags "Fuseholder 5x20 closed vertical Bulgin FX0456 Sicherungshalter ")
	(property "Reference" "REF**"
		(at 5.25 -7.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "Fuseholder_Cylinder-5x20mm_Bulgin_FX0456_Vertical_Closed"
		(at 5.08 8.89 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "S"
		(at 8.38 2.67 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at 5.25 -7.25 0)
		(layer "F.Fab")
	)
	(fp_text user "F"
		(at 1.78 -2.29 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0.08 -5)
		(size 2.2 2.2)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 0.08 5)
		(size 2.2 2.2)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 10.08 -5)
		(size 2.2 2.2)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 10.08 5)
		(size 2.2 2.2)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 3 3)
		(drill 1.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 10.16 0)
		(size 3 3)
		(drill 1.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Fuse.3dshapes/Fuseholder_Cylinder-5x20mm_Bulgin_FX0456_Vertical_Closed.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
