(footprint "Fuseholder_Cylinder-5x20mm_EATON_HBV_Vertical_Closed"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "5 mm x 20 mm fuse holders; Vertical w/ Stability Pins; 250V; 6.3-16A (http://www.cooperindustries.com/content/dam/public/bussmann/Electronics/Resources/product-datasheets/Bus_Elx_DS_2118_HB_PCB_Series.pdf)")
	(tags "fuse holder vertical 5x20mm")
	(property "Reference" "REF**"
		(at 5 -8.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Fuseholder_Cylinder-5x20mm_EATON_HBV_Vertical_Closed"
		(at 5 8.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 5 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0 -5)
		(size 2.54 2.54)
		(drill 2.54)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 0 5)
		(size 2.54 2.54)
		(drill 2.54)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 10 -5)
		(size 2.54 2.54)
		(drill 2.54)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 10 5)
		(size 2.54 2.54)
		(drill 2.54)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 10 0)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Fuse.3dshapes/Fuseholder_Cylinder-5x20mm_EATON_HBV_Vertical_Closed.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
