(footprint "Fuseholder_Cylinder-5x20mm_Schurter_FAB_0031-355x_Horizontal_Closed"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Fuseholder 5x20mm horizontal Shurter model FAB, Suitable for order numbers 0031.3551 and 0031.3558  (https://www.schurter.com/bundles/snceschurter/epim/_ProdPool_/newDS/en/typ_FAB.pdf)")
	(tags "Fuseholder 5x20mm closed horizontal")
	(property "Reference" "REF**"
		(at 13.125 -7 0)
		(layer "F.SilkS")
	)
	(property "Value" "Fuseholder_Cylinder-5x20mm_Schurter_FAB_0031-355x_Horizontal_Closed"
		(at 13.125 8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 13 5.25 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2.5 2.5)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 10 0)
		(size 2.5 2.5)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Fuse.3dshapes/Fuseholder_Cylinder-5x20mm_Schurter_FAB_0031-355x_Horizontal_Closed.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
