(footprint "Fuseholder_Cylinder-5x20mm_Schurter_FPG4_Vertical_Closed"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Shock-Safe Fuseholder, 5 x 20 mm, Slotted Cap/Fingergrip, vertical, IEC 60335-1; 250VAC/10A VDE; 500V/16A UL/CSA (https://us.schurter.com/bundles/snceschurter/epim/_ProdPool_/newDS/en/typ_FPG4.pdf)")
	(tags "fuse holder vertical 5x20mm")
	(property "Reference" "REF**"
		(at 3.81 -5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Fuseholder_Cylinder-5x20mm_Schurter_FPG4_Vertical_Closed"
		(at 3.81 10 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 3.81 2.54 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2.35 2.35)
		(drill 1.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 5.08)
		(size 2.35 2.35)
		(drill 1.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 7.62 0)
		(size 2.35 2.35)
		(drill 1.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 7.62 5.08)
		(size 2.35 2.35)
		(drill 1.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Fuse.3dshapes/Fuseholder_Cylinder-5x20mm_Schurter_FPG4_Vertical_Closed.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
