(footprint "Fuseholder_Cylinder-5x20mm_Schurter_FUP_0031.2510_Horizontal_Closed"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Shock-Safe closed Fuseholder, Schurter FUP Series, 5.0 x 20mm, Slotted Cap, horizontal, 500 VAC 4W/16A (VDE), 600V 30A (UL/CSA), order numbers: 0031.2510 (0031.2500 + 0031.2323), http://www.schurter.ch/bundles/snceschurter/epim/_ProdPool_/newDS/en/typ_FUP.pdf")
	(tags "Fuseholder 5x20mm horizontal closed")
	(property "Reference" "REF**"
		(at 0 -8.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Fuseholder_Cylinder-5x20mm_Schurter_FUP_0031.2510_Horizontal_Closed"
		(at 24 10.75 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 23.75 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 40.64 0)
		(size 2.6 2.6)
		(drill 2.6)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 4 2.5)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 10.16 -7.62)
		(size 4 2.5)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 10.16 7.62)
		(size 4 2.5)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Fuse.3dshapes/Fuseholder_Cylinder-5x20mm_Schurter_FUP_0031.2510_Horizontal_Closed.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
