(footprint "Fuseholder_Cylinder-5x20mm_Schurter_OGN-SMD_Horizontal_Open"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Fuseholder horizontal open, 5x20mm, 500V, 16A (https://us.schurter.com/bundles/snceschurter/epim/_ProdPool_/newDS/en/typ_OGN-SMD.pdf)")
	(tags "Fuseholder horizontal open 5x20 Schurter 0031.8221")
	(property "Reference" "REF**"
		(at 0 -6.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "Fuseholder_Cylinder-5x20mm_Schurter_OGN-SMD_Horizontal_Open"
		(at 0 6.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -8.5 0)
		(size 6 6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at 8.5 0)
		(size 6 6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Fuse.3dshapes/Fuseholder_Cylinder-5x20mm_Schurter_OGN-SMD_Horizontal_Open.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
