(footprint "Fuseholder_Cylinder-6.3x32mm_Schurter_0031-8002_Horizontal_Open"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Fuseholder, horizontal, open, 6.3x32, Schurter, 0031.8002, https://www.schurter.com/en/datasheet/typ_OG__Holder__6.3x32.pdf")
	(tags "Fuseholder horizontal open 6.3x32 Schurter 0031.8002")
	(property "Reference" "REF**"
		(at 18.85 -8.65 0)
		(layer "F.SilkS")
	)
	(property "Value" "Fuseholder_Cylinder-6.3x32mm_Schurter_0031-8002_Horizontal_Open"
		(at 18.95 8.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 19.5 6.5 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 18.75 0)
		(size 3.2 3.2)
		(drill 3.2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole oval
		(at 0 0)
		(size 3.25 6)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 37.5 0)
		(size 3.25 6)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Fuse.3dshapes/Fuseholder_Cylinder-6.3x32mm_Schurter_0031-8002_Horizontal_Open.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
