(footprint "Heatsink_125x35x50mm_3xFixationM3"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Heatsink, 125x35x50mm, 3 fixation holes 3.2mm")
	(tags "heatsink")
	(property "Reference" "REF**"
		(at 0 -34 0)
		(layer "F.SilkS")
	)
	(property "Value" "Heatsink_125x35x50mm_3xFixationM3"
		(at 0 4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0.003 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -48 0)
		(size 3.2 3.2)
		(drill 3.2)
		(layers "*.Cu" "*.SilkS" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 0 0)
		(size 3.2 3.2)
		(drill 3.2)
		(layers "*.Cu" "*.SilkS" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 48.006 0)
		(size 3.2 3.2)
		(drill 3.2)
		(layers "*.Cu" "*.SilkS" "*.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Heatsink.3dshapes/Heatsink_125x35x50mm_3xFixationM3.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
