(footprint "Heatsink_35x26mm_1xFixation3mm_Fischer-SK486-35"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Heatsink, 35mm x 26mm, 1x Fixation 3mm, Fischer SK486-35")
	(tags "heatsink")
	(property "Reference" "REF**"
		(at -8.54 -9.42 0)
		(layer "F.SilkS")
	)
	(property "Value" "Heatsink_35x26mm_1xFixation3mm_Fischer-SK486-35"
		(at -8.54 8.08 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at -8.54 -6.67 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 6.49732 6.49732)
		(drill 3.0988)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Heatsink.3dshapes/Heatsink_35x26mm_1xFixation3mm_Fischer-SK486-35.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
