(footprint "Heatsink_AAVID_573300D00010G_TO-263"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Heatsink, 12.70mm x 26.16mm x 10.16, SMD, 18K/W, TO-263, D2 Pak, https://www.shopaavid.com/Product/573300D00000G")
	(tags "Heatsink AAVID TO-263 D2 Pak")
	(property "Reference" "REF**"
		(at 0 -8 0)
		(layer "F.SilkS")
	)
	(property "Value" "Heatsink_AAVID_573300D00010G_TO-263"
		(at 0 8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "Drain Pad"
		(at -1.32 -1.94 0)
		(layer "Dwgs.User")
	)
	(fp_text user "Recommended"
		(at 0.24 -4.84 0)
		(layer "Dwgs.User")
	)
	(fp_text user "Heat Spreader"
		(at 0.32 -3.39 0)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0.75 0.07 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -6.92 0)
		(size 1.85 13.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd rect
		(at 6.92 0)
		(size 1.85 13.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Heatsink.3dshapes/Heatsink_AAVID_573300D00010G_TO-263.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
