(footprint "Heatsink_Fischer_FK24413DPAK_23x13mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "23x13 mm SMD heatsink for TO-252 TO-263 TO-268, https://www.fischerelektronik.de/pim/upload/fischerData/cadpdf/base/fk_244_13_d_pak.pdf")
	(tags "heatsink TO-252 TO-263 TO-268")
	(property "Reference" "REF**"
		(at -9.5 -7.5 180)
		(layer "F.SilkS")
	)
	(property "Value" "Heatsink_Fischer_FK24413DPAK_23x13mm"
		(at 0 8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "H10mm"
		(at 9.5 0 90)
		(layer "Cmts.User")
	)
	(fp_text user "H10mm"
		(at -9.5 0 90)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -6.2 0 180)
		(size 3.25 13.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "1" smd rect
		(at 6.2 0)
		(size 3.25 13.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Heatsink.3dshapes/Heatsink_Fischer_FK24413DPAK_23x13mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
