(footprint "Heatsink_SheetType_50x7mm_2Fixations"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Heatsink, Sheet type, 50x7mm, 2 fixations (solder),")
	(tags "Heatsink sheet")
	(property "Reference" "REF**"
		(at 0 -8 0)
		(layer "F.SilkS")
	)
	(property "Value" "Heatsink_SheetType_50x7mm_2Fixations"
		(at 1.27 5.08 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_mask_margin 0.2)
	(attr through_hole)
	(fp_text user "M3"
		(at -14.605 -4.826 0)
		(layer "F.SilkS")
	)
	(fp_text user "M3"
		(at 14.605 -4.953 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -22.606 0)
		(size 5.00126 5.00126)
		(drill 2.49936)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 22.606 0)
		(size 5.00126 5.00126)
		(drill 2.49936)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Heatsink.3dshapes/Heatsink_SheetType_50x7mm_2Fixations.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
