(footprint "L_APV_APH1770"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Inductor, APV, APH1770, 17.45x17.15x6.7mm, (http://en.apvind.com/public/upload/20240408/996aafa961154ed753e4983e7eb80fa7.pdf), generated with kicad-footprint-generator gen_inductor.py")
	(tags "Inductor molded power shielded")
	(property "Value" "L_APV_APH1770"
		(at 0 9.575 0)
		(layer "F.Fab")
	)
	(property "Reference" "REF**"
		(at 0 -9.575 0)
		(layer "F.SilkS")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -7.35 0)
		(size 3.5 12.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.071429)
	)
	(pad "2" smd roundrect
		(at 7.35 0)
		(size 3.5 12.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.071429)
	)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_APV_APH1770.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
