(footprint "L_Abracon_ASPI-0425"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Inductor, Abracon, ASPI-0425, 4.0x4.0x2.5mm, (https://abracon.com/Magnetics/new/ASPI-0425.pdf), generated with kicad-footprint-generator gen_inductor.py")
	(tags "Inductor power shielded low-profile")
	(property "Value" "L_Abracon_ASPI-0425"
		(at 0 3 0)
		(layer "F.Fab")
	)
	(property "Reference" "REF**"
		(at 0 -3 0)
		(layer "F.SilkS")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -1.525 0)
		(size 1.5 3.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.166667)
	)
	(pad "2" smd roundrect
		(at 1.525 0)
		(size 1.5 3.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.166667)
	)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Abracon_ASPI-0425.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
