(footprint "L_Changjiang_FXL1340"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Inductor, Changjiang, FXL1340, 12.9x12.8x4.0mm, (https://www.lcsc.com/datasheet/lcsc_datasheet_2404260921_cjiang--Changjiang-Microelectronics-Tech-FXL0420-2R2-M_C167206.pdf), generated with kicad-footprint-generator gen_inductor.py")
	(tags "Inductor power shielded cjiang fxl")
	(property "Value" "L_Changjiang_FXL1340"
		(at 0 7.4 0)
		(layer "F.Fab")
	)
	(property "Reference" "REF**"
		(at 0 -7.4 0)
		(layer "F.SilkS")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -5.625 0)
		(size 3.25 5.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.076923)
	)
	(pad "2" smd roundrect
		(at 5.625 0)
		(size 3.25 5.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.076923)
	)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Changjiang_FXL1340.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
