(footprint "L_Chilisin_BMRx00050515"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Inductor, Chilisin, BMRx00050515, 5.7x5.4x1.5mm, (https://www.chilisin.com/upload/media/product/power/file/BMRx_Series.pdf), generated with kicad-footprint-generator gen_inductor.py")
	(tags "Inductor bmrx mchi")
	(property "Value" "L_Chilisin_BMRx00050515"
		(at 0 3.7 0)
		(layer "F.Fab")
	)
	(property "Reference" "REF**"
		(at 0 -3.7 0)
		(layer "F.SilkS")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -2.05 0)
		(size 1.9 2.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.131579)
	)
	(pad "2" smd roundrect
		(at 2.05 0)
		(size 1.9 2.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.131579)
	)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Chilisin_BMRx00050515.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
