(footprint "L_Coilcraft_LPS3010"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Shielded Power Inductor SMD 3x3x1mm, Coilcraft LPS3010, https://www.coilcraft.com/pdfs/lps3010.pdf")
	(tags "inductor low profile")
	(property "Reference" "REF**"
		(at 0 -2.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_Coilcraft_LPS3010"
		(at 0 2.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd custom
		(at -1.27 0)
		(size 0.76 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.76 -0.825) (xy 0.38 -0.51) (xy 0.38 0.51) (xy 0.76 0.825) (xy 0.76 1.525) (xy -0.125 1.525)
					(xy -0.38 1.27) (xy -0.38 -1.27) (xy -0.125 -1.525) (xy 0.76 -1.525)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd custom
		(at 1.27 0 180)
		(size 0.76 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.76 -0.825) (xy 0.38 -0.51) (xy 0.38 0.51) (xy 0.76 0.825) (xy 0.76 1.525) (xy -0.125 1.525)
					(xy -0.38 1.27) (xy -0.38 -1.27) (xy -0.125 -1.525) (xy 0.76 -1.525)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Coilcraft_LPS3010.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
