(footprint "L_Coilcraft_LPS4414"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SMD Inductor Coilcraft LPS4414, https://www.coilcraft.com/getmedia/fa8805ca-b278-4819-915a-b5cf632f0239/lps4414.pdf")
	(tags "L Coilcraft LPS4414")
	(property "Reference" "REF**"
		(at 0 -3.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_Coilcraft_LPS4414"
		(at 0 3.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd custom
		(at -1.9875 0)
		(size 0.5 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.3625 -0.7) (xy 1.2375 -1.575) (xy 1.2375 -2.35) (xy 0.4875 -2.35) (xy -0.3625 -1.5) (xy -0.3625 1.5)
					(xy 0.4875 2.35) (xy 1.2375 2.35) (xy 1.2375 1.575) (xy 0.3625 0.7)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd custom
		(at 1.9875 0)
		(size 0.5 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.3625 -0.7) (xy -1.2375 -1.575) (xy -1.2375 -2.35) (xy -0.4875 -2.35) (xy 0.3625 -1.5) (xy 0.3625 1.5)
					(xy -0.4875 2.35) (xy -1.2375 2.35) (xy -1.2375 1.575) (xy -0.3625 0.7)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Coilcraft_LPS4414.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
