(footprint "L_Coilcraft_LPS5030"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Shielded Power Inductor SMD, Coilcraft LPS5030, https://www.coilcraft.com/pdfs/lps5030.pdf, StepUp generated footprint")
	(tags "inductor")
	(property "Reference" "REF**"
		(at 0 -3.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_Coilcraft_LPS5030"
		(at 0 3.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd custom
		(at -2.2275 0)
		(size 1.055 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.4675 -1.7) (xy 0.5275 -0.8445) (xy 0.5275 0.8445) (xy 1.4675 1.7) (xy 1.4675 2.755) (xy 0.5275 2.755)
					(xy -0.5275 1.7) (xy -0.5275 -1.7) (xy 0.5275 -2.755) (xy 1.4675 -2.755)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd custom
		(at 2.2275 0)
		(size 1.055 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.5275 -1.7) (xy 0.5275 1.7) (xy -0.5275 2.755) (xy -1.4675 2.755) (xy -1.4675 1.7) (xy -0.5275 0.8445)
					(xy -0.5275 -0.8445) (xy -1.4675 -1.7) (xy -1.4675 -2.755) (xy -0.5275 -2.755)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Coilcraft_LPS5030.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
