(footprint "L_CommonModeChoke_Murata_DLW5BTMxxxSQ2x_5x5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Wire Wound Chip Common Mode Choke Coil SMD, Murata DLW5BTxxxSQ2x, https://www.murata.com/products/productdata/8796762701854/EFLC0020.pdf, manual footprint")
	(tags "inductor common mode choke")
	(property "Reference" "REF**"
		(at 0 -3.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_CommonModeChoke_Murata_DLW5BTMxxxSQ2x_5x5mm"
		(at 0 3.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd custom
		(at -1.5 -0.95 270)
		(size 1 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -1.8 0.85) (xy 0.5 0.85) (xy 0.5 -0.85) (xy -0.5 -0.85) (xy -0.5 0.15) (xy -1.8 0.15)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd custom
		(at -1.5 0.95 270)
		(size 1 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.8 0.85) (xy -0.5 0.85) (xy -0.5 -0.85) (xy 0.5 -0.85) (xy 0.5 0.15) (xy 1.8 0.15)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "3" smd custom
		(at 1.5 0.95 90)
		(size 1 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -1.8 0.85) (xy 0.5 0.85) (xy 0.5 -0.85) (xy -0.5 -0.85) (xy -0.5 0.15) (xy -1.8 0.15)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "4" smd custom
		(at 1.5 -0.95 90)
		(size 1 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.8 0.85) (xy -0.5 0.85) (xy -0.5 -0.85) (xy 0.5 -0.85) (xy 0.5 0.15) (xy 1.8 0.15)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_CommonModeChoke_Murata_DLW5BTMxxxSQ2x_5x5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
