(footprint "L_CommonModeChoke_Wuerth_WE-SL5"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "WE-SL5 SMT Common Mode Line Filter, 9.5x8.3mm, height 5mm, https://www.we-online.com/components/products/datasheet/744273222.pdf")
	(tags "SMT Common Mode Line Filter")
	(property "Reference" "REF**"
		(at 0 -5.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_CommonModeChoke_Wuerth_WE-SL5"
		(at 0 5.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -3.8 -3.1 180)
		(size 2.7 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.09259259259)
	)
	(pad "2" smd roundrect
		(at -3.8 3.1 180)
		(size 2.7 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.09259259259)
	)
	(pad "3" smd roundrect
		(at 3.8 3.1 180)
		(size 2.7 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.09259259259)
	)
	(pad "4" smd roundrect
		(at 3.8 -3.1 180)
		(size 2.7 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.09259259259)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_CommonModeChoke_Wuerth_WE-SL5.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
