(footprint "L_CommonMode_Delevan_4222"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "API Delevan, Surface Mount Common Mode Bead, 4222 4222R, http://www.delevan.com/seriesPDFs/4222.pdf")
	(tags "surface mount common mode bead")
	(property "Reference" "REF**"
		(at 0 -4 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_CommonMode_Delevan_4222"
		(at 0 4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -3.75 -1.27)
		(size 3 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -3.75 1.27)
		(size 3 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 3.75 1.27)
		(size 3 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 3.75 -1.27)
		(size 3 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_CommonMode_Delevan_4222.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
