(footprint "L_Eaton_MCL2012V1"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Inductor, Eaton, MCL2012V1, 2.0x1.2x0.9mm, (https://eu.mouser.com/datasheet/2/87/eaton-mcl2012v1-multilayer-chip-inductor-data-shee-1622891.pdf), generated with kicad-footprint-generator gen_inductor.py")
	(tags "Inductor ferrite multilayer power")
	(property "Value" "L_Eaton_MCL2012V1"
		(at 0 1.8 0)
		(layer "F.Fab")
	)
	(property "Reference" "REF**"
		(at 0 -1.8 0)
		(layer "F.SilkS")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.8 0)
		(size 1.2 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.208333)
	)
	(pad "2" smd roundrect
		(at 0.8 0)
		(size 1.2 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.208333)
	)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Eaton_MCL2012V1.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
