(footprint "L_Fastron_PISN_Handsoldering"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Choke, Drossel, PISN, SMD, Fastron,")
	(tags "Choke Drossel PISN SMD Fastron ")
	(property "Reference" "REF**"
		(at 0 -6.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_Fastron_PISN_Handsoldering"
		(at 0 6.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.05 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at 5.67 -0.01)
		(size 4 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -5.67 0.01)
		(size 4 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Fastron_PISN.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
