(footprint "L_Ferrocore_DLG-0403"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr " Ferrocore DLG-0403 unshielded SMD power inductor, 4.5x4.0x3.2mm, https://www.tme.eu/Document/bda580f72a60a2225c2f6576c2740ae1/dlg-0504.pdf")
	(tags "smd inductor dlg-0403")
	(property "Reference" "REF**"
		(at 0 -3.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_Ferrocore_DLG-0403"
		(at 0 3.2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.625 0)
		(size 1.75 4.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 1.625 0)
		(size 1.75 4.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Ferrocore_DLG-0403.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
