(footprint "L_KOHERelec_MDA5030"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Inductor, KOHERelec, MDA5030, 5.2x5.2x2.8mm, (http://www.kohergroup.com/template/default/pdf/MDA5030.pdf), generated with kicad-footprint-generator gen_inductor.py")
	(tags "Inductor high-current power shielded")
	(property "Value" "L_KOHERelec_MDA5030"
		(at 0 3.6 0)
		(layer "F.Fab")
	)
	(property "Reference" "REF**"
		(at 0 -3.6 0)
		(layer "F.SilkS")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -2.2 0)
		(size 1.6 2.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.15625)
	)
	(pad "2" smd roundrect
		(at 2.2 0)
		(size 1.6 2.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.15625)
	)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_KOHERelec_MDA5030.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
