(footprint "L_Pulse_PA4332"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Inductor, Pulse, PA4332, 4.2x4.2x2.0mm, (https://productfinder.pulseelectronics.com/api/open/part-attachments/datasheet/pa4332.222nlt), generated with kicad-footprint-generator gen_inductor.py")
	(tags "Inductor Pulse SMT PA4332")
	(property "Value" "L_Pulse_PA4332"
		(at 0 3.1 0)
		(layer "F.Fab")
	)
	(property "Reference" "REF**"
		(at 0 -3.1 0)
		(layer "F.SilkS")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -1.5 0)
		(size 1.1 3.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(pad "2" smd roundrect
		(at 1.5 0)
		(size 1.1 3.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Pulse_PA4332.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
