(footprint "L_SOREDE_SNR.1050_10x10x5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Sorede 10x10x5mm Power Inductor, https://datasheet.lcsc.com/lcsc/2201141530_SOREDE-SNR-1050-TYD4R7MT00_C2942304.pdf")
	(tags "Inductor Sorede SNR ")
	(property "Reference" "REF**"
		(at 0 -6.1 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_SOREDE_SNR.1050_10x10x5mm"
		(at 0 6.15 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -4.1 0)
		(size 2 5.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "2" smd roundrect
		(at 4.1 0)
		(size 2 5.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_SNR.1050_10x10x5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
