(footprint "L_Sagami_CWR1277C"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Sagami power inductor, CWR1242C, H=7.7mm (http://www.sagami-elec.co.jp/file/16Car_SMDCwr.pdf)")
	(tags "inductor sagami cwr12xx smd")
	(property "Reference" "REF**"
		(at 0 -7.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_Sagami_CWR1277C"
		(at 0 7.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -5.35 0)
		(size 2.5 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd rect
		(at 0 5.35)
		(size 3.6 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0 -5.35)
		(size 3.6 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 5.35 0)
		(size 2.5 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Sagami_CWR1277C.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
