(footprint "L_TDK_MLZ1608"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Inductor, TDK, MLZ1608, 1.6x0.8x0.8mm, ( \"https://product.tdk.com/system/files/dam/doc/product/inductor/inductor/smd/catalog/inductor_commercial_decoupling_mlz1608_en.pdf\"), generated with kicad-footprint-generator gen_inductor.py")
	(tags "Inductor MLZ")
	(property "Value" "L_TDK_MLZ1608"
		(at 0 1.4 0)
		(layer "F.Fab")
	)
	(property "Reference" "REF**"
		(at 0 -1.4 0)
		(layer "F.SilkS")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.4 0)
		(size 0.6 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at 0.4 0)
		(size 0.6 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_TDK_MLZ1608.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
