(footprint "L_TDK_SLF7045"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Inductor, TDK, SLF7045, 7.0mmx7.0mm (Script generated with StandardBox.py) (https://product.tdk.com/info/en/document/catalog/smd/inductor_commercial_power_slf7045_en.pdf)")
	(tags "Inductor TDK_SLF7045")
	(property "Reference" "REF**"
		(at -1 -4.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_TDK_SLF7045"
		(at 0 4.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -3.15 0)
		(size 1.5 2.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at 3.15 0)
		(size 1.5 2.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_TDK_SLF7045.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
